 LABORATORI D'ENVOL PARAGLIDING
 Paragliders and parachutes design program

 LEparagliding 3.29   version "Jardins"                                         
 2026-08-18

 Pere Casellas
 pere@laboratoridenvol.com
 GNU General Public License 3.0 http://www.gnu.org

 01-Planform read
 02-Airfoils read
 03-Anchors position read
 04-Airfoil holes read
 05-Skin tension read
 06-Sewing allowances read
 07-Marks read
 08-Calage read
 09-Lines read
 10-Brakes read
 11-Ramifications read
 12-H V VH ribs read
 16-Intrados colors read
 17-Aditional rib points read
 18-Elastic lines corrections read
 19-DXF layer names read
 20-DXF mark types read
 21-Joncs definition read
 22-Nose mylars definition read
 23-Tab reinforcements definition read
 24-General 2D DXF options read
 25-General 3D DXF options read
 26-Glue vents read
 27-Special wingtip read
 28-Parameters for calage variation read
 29-3D-Shaping read
 30-Airfoil modification read
 31-New skin tension read
 32-Parameters for part separation read
 33-Parameters for detailed risers read
 34-Parameters for lines characteristics table read
 35-Parameters for solve equilibrium read
 36-Parameters for xflr5 analysis read
 37-Some special parameters read
 38-HVR holes read
 39-HVR position parameters read
 All data read! Calculus start...please wait a moment

 Area = 18.00 m2

 Total line length =  239.09 m

 OK, paraglider calculated!

 Please open the following files:

    leparagliding.dxf
    lep-3d.dxf
    lep-3d-surfaces.dxf
    lep-out.txt
    lines.txt
    run-log.txt
    ../stl/lep-3d-surfaces.stl
    ../stl/lep-3d-surfaces.scad

