Very important! First of all, print the 4-sheet mosaic "00_mosaic_calibration_A4.pdf" to verify that the printer is properly calibrated. 
When printing the rest of the sheets, keep in mind that the central square of each sheet must be 50x50 mm.